# i3blocks config file
#
# Please see man i3blocks for a complete reference!
# The man page is also hosted at http://vivien.github.io/i3blocks
#
# List of valid properties:
#
# align
# color
# command
# full_text
# instance
# interval
# min_width
# name
# separator
# separator_block_width
# short_text
# signal
# urgent

# Global properties
#
# The top properties below are applied to every block, but can be overridden.
# Each block command defaults to the script name to avoid boilerplate.
command=${HOME}/.i3blocks/$name
separator_block_width=11
markup=pango

#[window_title]
#command=echo $(xdotool getactivewindow getwindowname)
#interval=1

# CPU usage
#
# The script may be called with -w and -c switches to specify thresholds,
# see the script for details.
[cpu_usage]
interval=1
#min_width= 99.99%
#separator=false

[load_average]
interval=5

# Temperature
#
# Support multiple chips, though lm-sensors.
# The script may be called with -w and -c switches to specify thresholds,
# see the script for details.
[temperature]
#instance=coretemp-isa-0000
interval=3
#separator=false
#
#[temperature]
#instance=radeon-pci-0300
#interval=3
# Memory usage
#
# The type defaults to "mem" if the instance is not specified.
[memory]
#separator=false
interval=2
#min_width=RAM 99.99%

#[memory]
#instance=swap
##separator=false
#interval=2
##min_width=swap 99.9%

# Disk usage
#
# The directory defaults to $HOME if the instance is not specified.
# The script may be called with a optional argument to set the alert
# (defaults to 10 for 10%).
#[disk]
#instance=/
#interval=30
#separator=false

#[disk]
#instance=/mnt/data
#interval=30

[internet]
interval=30
separator=false

[bandwidth]
interval=2

# Network interface monitoring
#
# If the instance is not specified, use the interface used for default route.
# The address can be forced to IPv4 or IPv6 with -4 or -6 switches.
#[iface]
#instance=wlp1s0
#interval=10
#separator=false

#[public_ip]
#interval=60
#separator=false

[vpn]
interval=30
separator=false

#[bandwidth]
#interval=1
#markup=none

# Packages to update
[updates]
interval=600


#[wifi]
#instance=wlp1s0
#interval=3
#separator=false

#[bandwidth]
#instance=wlp1s0
#interval=1
#min_width=d 999K u 999K

#[bandwidth]
#instance=enp0s31f6
#interval=1
#min_width=IN 999K OUT 999K


# Battery indicator
#
# The battery instance defaults to 0.
#[battery]
#instance=0
#interval=5

#[batterybar]
#[battery]
#interval=10
#min_width="bat ██████"

# Generic media player support
#
# This displays "ARTIST - SONG" if a music is playing.
# Supported players are: spotify, vlc, audacious, xmms2, mplayer, and others.
[mpd]
#instance=spotify
interval=1
signal=13
#markup=none

# OpenVPN support
#
# Support multiple VPN, with colors.
#[openvpn]
#interval=20

# Volume indicator
#
# The first parameter sets the step (and units to display)
# The second parameter overrides the mixer selection
# See the script for details.
[volume]
instance=vol
#instance=PCM
interval=once
signal=10
separator=false

[volume]
instance=mic
#instance=PCM
interval=once
signal=10


# Key indicators
#
# Add the following bindings to i3 config file:
#
# bindsym --release Caps_Lock exec pkill -SIGRTMIN+11 i3blocks
# bindsym --release Num_Lock  exec pkill -SIGRTMIN+12 i3blocks
[dunst]
interval=60

[bepo]
interval=60

[beep]
interval=once
signal=14
separator=false

[keyindicator]
instance=Caps
interval=once
signal=11
separator=false

[keyindicator]
instance=Num
interval=once
signal=12
# Date Time
#
[time]
interval=1
markup=none
